**Parliamentary Counsel Committee**

**Model Work Health and Safety (Blood Lead Removal Levels) Amendment Regulations 2018–Model Provisions**

made under the

*Model Work Health and Safety Bill*

|  |  |
| --- | --- |
| Contents |  |
|  |  | Page |
| [1](#_bookmark0) | [Short title . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .](#_bookmark1) | [2](#_bookmark1) |
| [2](#_bookmark2) | [Regulations amended . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .](#_bookmark3) | [2](#_bookmark3) |
| [3](#_bookmark4) | [Amendment of r 394 (Meaning of lead risk work) . . . . . . . . . . . .](#_bookmark5) | [2](#_bookmark5) |
| [4](#_bookmark6) | [Amendment of r 407 (Frequency of biological monitoring) . . . . .](#_bookmark7) | [2](#_bookmark7) |
| [5](#_bookmark8) | [Amendment of r 415 (Removal of worker from lead risk work) . .](#_bookmark9) | [3](#_bookmark9) |
| [6](#_bookmark10) | [Amendment of r 417 (Return to lead risk work after removal) . . .](#_bookmark11) | [3](#_bookmark11) |

Model Work Health and Safety (Blood Lead Removal Levels) Amendment Regulations 2018–Model Provisions

[s 1]

1. **Short title**

This Regulation may be cited as the *Model Work Health and Safety (Blood Lead Removal Levels) Amendment Regulations 2018–Model Provisions*.

1. **Regulations amended**

This Regulation amends the *Model Work Health and Safety Regulations*.

1. **Amendment of r 394 (Meaning of *lead risk work*)**

(1) Regulation 394(a), ‘10µg/dL (0.48µmol/L)’—

*omit, insert*—

5µg/dL (0.24µmol/L)

(2) Regulation 394(b), ‘30µg/dL (1.45µmol/L)’—

*omit, insert*—

20µg/dL (0.97µmol/L)

1. **Amendment of r 407 (Frequency of biological monitoring)**

(1) Regulation 407(1)(a)(i), ‘30µg/dL (1.45µmol/L)’—

*omit, insert*—

10µg/dL (0.48µmol/L)

(2) Regulation 407(1)(a)(ii), ‘30µg/dL (1.45µmol/L) or more but less than 40µg/dL (1.93µmol/L)’—

*omit, insert*—

10µg/dL (0.48µmol/L) or more but less than 20µg/dL (0.97µmol/L)

(3) Regulation 407(1)(a)(iii), ‘40µg/dL (1.93µmol/L)’—

*omit, insert*—

20µg/dL (0.97µmol/L)

Page 2

Model Work Health and Safety (Blood Lead Removal Levels) Amendment Regulations

2018–Model Provisions

[s 5]

(4) Regulation 407(1)(b)(i), ‘10µg/dL (0.48µmol/L)’—

*omit, insert*—

5µg/dL (0.24µmol/L)

(5) Regulation 407(1)(b)(ii), ‘10µg/dL (0.48µmol/L) or more’—

*omit, insert*—

5µg/dL (0.24µmol/L) or more but less than 10µg/dL (0.48µmol/L)

1. **Amendment of r 415 (Removal of worker from lead risk work)**

(1) Regulation 415(1)(a)(i), ‘50µg/dL (2.42µmol/L)’—

*omit, insert*—

30µg/dL (1.45µmol/L)

(2) Regulation 415(1)(a)(ii) and (iii)—

*omit, insert*—

(ii) for females of reproductive capacity— 10µg/dL (0.48µmol/L).

1. **Amendment of r 417 (Return to lead risk work after removal)**

(1) Regulation 417(3)(a)(i), ‘40µg/dL (1.93µmol/L)’—

*omit, insert*—

20µg/dL (0.97µmol/L)

(2) Regulation 417(3)(a)(ii), ‘10µg/dL (0.48µmol/L)’—

*omit, insert*—

5µg/dL (0.24µmol/L)

Page 3