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[bookmark: _Toc239435925]About this checklist
This checklist can assist with identifying slip, trip and fall hazards in the workplace. It covers some of the most common things you should check for. It is not intended to be a complete list, and you may modify or add additional items to suit your workplace needs. 
Industry standards, legislative requirements and guidelines may apply. More information for what is relevant in your jurisdiction is available from your WHS regulator.
[bookmark: _Toc239435926]How to use this checklist
If you answer ‘No’ to any of the questions, refer to the corresponding section in the ‘Hazards and risks’ chapter of this guide for ideas about what control measures may be suitable for your workplace. Some ways you can determine the answers to the questions include:
inspecting the physical workplace in person, both indoors and outdoors
observing workers to understand how work is carried out 
consulting workers, including a competent person and a Health and Safety Representative
checking industry guidance and standards to see if there is an objective measurement for “effective” or “adequate” in your industry, where relevant
referring to manufacturer’s instructions or consulting manufacturers, or
checking reports of incidents and near misses.
You should keep a copy of the completed checklist to refer to later. This will make it easier to keep track of how often control measures are being reviewed and whether they are working as expected.
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1. Internal Floors
	Check Item
	Yes
	No

	Floors are in good condition, level, and free from damage.
	☐	☐
	Floor surfaces provide adequate grip for expected conditions.
	☐	☐
	Changes in floor levels or surfaces are clearly visible.
	☐	☐
	No leaks, pooled liquids, tracked‑in water, or contamination.
	☐	☐
	Walkways are free from objects, cables, equipment or stored items.
	☐	☐

2. External Areas
	Check Item
	Yes
	No

	Pathways are stable, level, and well maintained.
	☐	☐
	External surfaces remain slip‑resistant when wet.
	☐	☐
	Drainage prevents pooling of water or mud.
	☐
	☐
	Grates, covers and outdoor surfaces are in good condition.
	☐	☐
	Vegetation is controlled so debris does not create hazards.
	☐	☐

3. Cleaning & Maintenance
	Check Item
	Yes
	No

	Cleaning methods suit the flooring material.
	☐	☐
	Spills are cleaned promptly using effective procedures.
	☐	☐
	Wet‑floor warning signs, barriers or exclusion zones are used correctly.
	☐	☐
	Maintenance issues (e.g. lighting, leaks, flooring damage) are identified and actioned quickly.
	☐	☐
	Drainage is adequate where liquids are used or stored.
	☐	☐

4. Housekeeping
	Check Item
	Yes
	No

	Accessways are clear, tidy, and free from clutter.
	☐	☐
	Adequate storage is located close to points of use.
	☐	☐
	Power outlets are positioned to avoid trailing cords.
	☐	☐
	Contractors follow the site’s housekeeping and cleaning expectations.
	☐	☐



5. Lighting
	Check Item
	Yes
	No

	Lighting is sufficient to identify slip, trip and fall hazards.
	☐	☐
	Step edges, ramps and transitions are clearly visible.
	☐	☐
	Glare, reflections and deep shadows are minimised.
	☐	☐
	Outdoor paths and carparks have adequate lighting during low light conditions.
	☐	☐

6. Stairs & Ramps
	Check Item
	Yes
	No

	Stairs and ramps meet design standards and are well maintained.
	☐	☐
	Step edges and ramp transitions are clearly marked.
	☐	☐
	Handrails are present, secure, continuous and easy to grip.
	☐	☐
	Surfaces provide suitable traction under expected conditions.
	☐	☐

7. Work Tasks
	Check Item
	Yes
	No

	Tasks allow workers to maintain balance and visibility of the path of travel.
	☐	☐
	Loads carried do not obstruct vision, especially on stairs or ramps.
	☐	☐
	Mechanical aids (trolleys, etc.) are appropriate for the surface and task.
	☐	☐
	Distractions (e.g. noise, lighting issues, multitasking) are minimised.
	☐	☐

8. Footwear
	Check Item
	Yes
	No

	Footwear is suitable, in good condition, and provides adequate grip.
	☐	☐
	Workers understand and follow the workplace footwear requirements.
	☐	☐

9. Training, Reporting and Supervision
	Check Item
	Yes
	No

	Workers are trained in slip, trip and fall risks, spill response and hazard reporting.
	☐	☐
	Training records are kept and reviewed when processes or equipment change.
	☐	☐
	Workers know how to report hazards, near misses and faulty equipment.
	☐	☐
	Supervision is appropriate for task risk level and worker experience.
	☐	☐


10. Psychosocial hazards
	Check Item
	Yes
	No

	Deadlines and quotas are realistic, with enough time to meet them safely.
	☐	☐
	Work assigned is a mix of fast / slow paced, and high / low concentration.
	☐	☐
	Rosters take into account total hours worked, shift length and timing (e.g. night or irregular hours).
	☐	☐
	Monitor for signs of fatigue.
	☐	☐
	Enough breaks for the type of work and the worker’s needs.
	☐	☐
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	Control measures needed

	

	

	

	

	

	

	

	Next steps: who, what, when
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